VOLLMER model CA2 200 fool flood CNC grinder for bandsaws.

Complete with second feed on back and central height adjustment off carrousel.

Year off construction: 1999, serial number 193.

Wheel diameter 250 mm pitch 6-120 mm and hook angle up to 40°

Can be used for corundum or CBN grinding disks.

We think its wise to recondition this machine (rust).

VOLLMER Model CAR 200 wassergekühlte CNC Schärfmaschine für Bandsägen.

Komplett mit 2. Drückfinger hinten und Zentrale Höheneinstellung der Karussell.

Baujahr 1999, Serien Nummer 193.

Schleifscheiben Durchmesser 250mm, Zahnteilung 6-120 mm und Schnittwinkel bis 40°.

Es können Korund oder CBN-Scheiben benützt werden.

Überholung = empfohlen (Verrostet)

VOLLMER type CAR 200 affûteuse CNC pour rubans large.

Complet avec 2° poussoir à l’arrière et réglage centralisé de la hauteur du carrousel.

Année 1999, numéro de série 193.

Diamètre meules 250, pas de denture 6-120 mm et angle d’attaque jusqu’à 40°.

La machine accepte des meules corindon ou borazon même diamantés.

Un reconditionnement est conseillé (rouille)

VOLLMER type CAR 200 CNC gestuurde slijpmachine voor brede bandzaagbladen.

Volledig met 2. Aanvoervinger achteraan en centrale hoogteinstelling van de carrousel.

Bouwjaar 1999; serienummer 193.

Slijpsteendoormeter 250, tandsteek 6-120 mm en snijhoek tot 40°.

De machine aanvaardt Korund slijpstenen of borazon, zelfs diamant.

Het lijkt nodig een volledige revisie te doen (roestvorming)